TI RTOS ROM Release Notes

February 8, 2018

# Description

TI RTOS ROM image for CC26X2V2 devices.

This ROM image comes from the 6.53.02.00 product and can be found in:

“packages/ti/sysbios/rom/cortexm/cc26x2v2/golden/CC26xx/rtos\_rom.elf”

TI RTOS functionality includes Hwi, Swi, Task, Clock, Event, Semaphore, Mailbox, HeapTrack, and HeapMem.

The complete list of APIs contained within the ROM image can be found in:

“packages/ti/sysbios/rom/cortexm/cc26x2v2/golden/CC26xx/rtos\_rom.txt”

# Release Information

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Target | CC26X2V2 | | | |
| Files | rtos\_rom.elf  rtos\_rom.elf.mem  TI\_RTOS\_ROM\_Release\_Notes.docx | | | |
| Memory Allocation |  | Start | End | Size/Used |
| ROM | 0x1002B400 | 0x1002FDED | 18,926 |
| RAM | 0x20000100 | 0x2000010B | 12 |
| FLASH | 0x00001000 | 0x00001000 | 0 |

# Configuration and Build Tools

XDC TOOLS = xdctools\_3\_50\_03\_33

PLATFORMS = platformprod-p03

# Build Files

avala-6\_53\_02\_00